# **Lab 3 - Task 3**

In this task, you will learn how the receiver in the stop and wait protocol passes data to the application layer. Remember that in the stop and wait protocol the receiver may receive duplicated packets, due to acknowledgements being lost and time outs. However, reliable transport protocols must ensure that all segments containing the message are passed to the application layer in order and without duplication.

**INSTRUCTIONS**

The MATLAB code in the window below is similar to that in Task 1. However, since we are interested in the operation of the receiver, we show the implementation of the function **receiver\_stopwait()** below the line

% receiver

In each iteration of the simulation, the receiver first checks if a packet has arrived during the current time slot using the function **receiver\_get\_packet()**. This function returns the packet (a 24 bit binary vector) if a packet has arrived or an empty matrix if no packet has arrived. If a packet has arrived, it extracts the first eight bits of the packet, which contain the sequence number of the packet, and sends them back to the sender as an **ACK** packet using the function **receiver\_send\_ack()**. Then, it adds the received packet to the list of received packets, called **receiver\_packet\_list**. Note that, when doing this, the initial code does not check whether the new packet is duplicated or not, i.e., whether the new packet has been received before. As a result, the message, **rx\_msg\_1**, reconstructed from **receiver\_packet\_list** by the function **reconstruct\_msg()** may have duplicated characters.

Your task is to filter out the duplicated packets from **receiver\_packet\_list** and to create a new list, called **revised\_packet\_list**, that will contain the packets in the correct order and without redundant items. The initial code contains an incorrect implementation of the filtering described in the lecture on the stop and wait protocol.

To help you check your result, the code will reconstruct the correct message from the **revised\_packet\_list** and save it to the variable **rx\_msg\_2**. Revise the code between the lines

% % % % Revise the following code % % % %

and

% % % % Do not change the code below % % % %

Please, do not change other parts of the code.